Filter:

Submit Search

### Step 1: Specifying the MPR range

You can specify the range from which to create Multi-Planar Reconstruction (MPR) images. If the MPR range is not specified, the entire series is used.

For an overview of MPR images, see About creating MPR images.

Setting the MPR start range

To set the MPR start range:

| 1. | Click the first image for creating MPR images.

| 2. | Click the Display Mode icon at the top of the viewport. The Display Mode icon indicates the types of images currently displayed. See Specifying the series viewing scope.

| 3. | From the menu that is displayed, point to Advanced, and then select Start MPR Range Marker.

Setting the MPR end range

To set the MPR end range:

| 1. | Click the last image for creating MPR images.

| 2. | Click the Display Mode icon at the top of the viewport.

| 3. | From the menu that is displayed, point to Advanced, and then select End MPR Range Marker.

Clearing the MPR range

To clear the MPR range:

| 1. | Click the viewport.

| 2. | Click the Display Mode icon at the top of the viewport.

| 3. | Form the menu that is displayed, point to Advanced, and then select Clear MPR Range Markers.

Related Topics

Your search for returned result(s).