Filter:

Submit Search

### Selecting the series display mode

Images have two series display modes.

Note: Cross-sectional images can also be displayed as multi-planar reconstruction (MPR) images. See Creating MPR images.

Available series display modes

The following table describes the available series display modes.

Series display mode | Meaning
Standard | Still images are displayed. You can scroll through a series in Standard mode, or jump to a specific image. See Navigating a series.
Cine | Images are displayed as a sequence of frames, as if you are viewing a cine clip. For details on cine clips, see Working with cine clips. Note: Series containing only one image cannot be displayed in Cine mode.

Steps for this task

To select the series display mode:

| 1. | Click the Display Mode icon at the top of the viewport. The Display Mode icon indicates the types of images currently displayed. See Specifying the series viewing scope.

Note: The Display Mode icon is not displayed if the series contains only one image.

| 2. | From the menu that is displayed, select the series display mode of your choice.

Related Topics

Your search for returned result(s).