Filter:

Submit Search

## About cine clips

A cine clip is a time-based image that contains a sequence of frames. Typically, cine clips are used in Ultrasound (US), Radio Fluoroscopy (RF), and X-Ray Angiography (XA) studies.

Indication of a cine clip

A cine clip is indicated by the thumbnail representing the series. See Thumbnail appearance.

Available cine clips display modes

Cine clips have two display modes. The following table describes the available cine clips display modes.

Cine clips display mode | Meaning
Cine | The cine clip is displayed as a sequence of frames. The chits at the top of the viewport are replaced by the Cine Playback control. See Viewing cine clips.
Standard | The cine clip is displayed as a series of still images. Displaying a cine clip in Standard mode enables you to manipulate a frame as if you would an image. See Working with images.

Steps for this task

To switch between the Cine mode and Standard mode:

| 1. | Click the Display Mode icon at the top of the viewport.

| 2. | From the menu that is displayed, select the cine clips display mode of your choice:

| • | Standard Mode

| • | Cine Mode

Your search for returned result(s).