Filter:

Submit Search

#### Selecting a subset

When you create MPR images, the Disc Advanced Viewerchecks for non-uniform images in the series. Images are considered non-uniform when they have the following properties:

| • | Different orientation, for example, an image in the series is displayed in a different position when compared to the rest of the series (for example, the image has been flipped or rotated).

| • | Different slice thickness

| • | Irregular spacing, which results in gaps between the slices.

Non-uniform images cannot be used to create MPR images. As a result, the Disc Advanced Viewer identifies subsets that contain uniform images. You can select the subset from which you want to create MPR images.

Steps for this task

To select a subset:

| 1. | In the Valid Image Subset Selection dialog box, click the subset from which you want to create MPR images.

If there are more than four subsets, you can page through the subsets, by clicking Next and Previous.

Note: The slider on top of each thumbnail indicates where the corresponding image is located within the series. To view a different image, drag the slider to a different position. Or, you can scroll through the subset, by placing the mouse pointer on the thumbnail and rotating the mouse wheel.

| 2. | Optionally, to view the information about the images in the subset, do the following:

| • | Click the subset, and then click Info.

| • | The Image Information dialog box is displayed. When you finish viewing the information, click Close.

| 3. | Click OK. The MPR images are created accordingly.

Your search for returned result(s).