Filter:

Submit Search

#### Calibrating monitors for life size image display

Displaying images at life size enables you to clearly visualize the anatomy at its physical size. The monitors are calibrated for life size image display at installation by Change Healthcare. You may also re-calibrate the monitors at anytime.

Restriction for calibrating monitors for life size image display

You must have the authority to calibrate monitors for life size image display. For details, contact your system administrator.

Prerequisite

You need a ruler that can be placed flat on the monitor.

Steps for this task

To calibrate a monitor at life size:

| 1. | Click the arrow beside the Zoom icon on the main toolbar.

| 2. | From the menu that is displayed, select Calibrate Monitor for Life Size.

The Life Size Monitor Calibration dialog box is displayed.

| 3. | Calibrate the monitor as follows:

| • | Specify the measurement unit you want to use for calibration. The available options are cm or inches.

| • | Drag the lower right corner of the Life Size Monitor Calibration dialog box, until the sides of the calibration box (the box that contains a circle) have the same length.

| • | Drag the calibration box, until the length of each side is the same as the indicated measurement (10 cm or 5 inches).

| 4. | Click Next.

| 5. | If the workstation has multiple monitors, the Life Size Monitor Calibration dialog box is displayed on the next monitor. Repeat steps 3-4 for each monitor.

| 6. | Click Finish.

Related Topics

Your search for returned result(s).